(module YAG_conn_audio_MJ352WC (layer F.Cu)
  (at 0 0)
  (fp_text reference MJ-352W-C (at 7 -7) (layer F.SilkS))
  (fp_text value CONN** (at 7 6.5) (layer F.SilkS))
  (pad 1 thru_hole oval (at 2 0) (size 2 2.5) (drill oval 0.6 1.5)
    (layers *.Cu *.Mask F.SilkS)
  )
  (pad 2 thru_hole oval (at 5 4.55) (size 2.5 2) (drill oval 1.5 0.6)
    (layers *.Cu *.Mask F.SilkS)
  )
  (pad 3 thru_hole oval (at 13.1 4) (size 2 2.5) (drill oval 0.6 1.5)
    (layers *.Cu *.Mask F.SilkS)
  )
  (pad 4 thru_hole oval (at 8.5 -3) (size 2.4 1.7) (drill oval 1.5 0.6)
    (layers *.Cu *.Mask F.SilkS)
  )
  (pad 5 thru_hole oval (at 9.9 -5.05) (size 2.4 1.7) (drill oval 1.5 0.6)
    (layers *.Cu *.Mask F.SilkS)
  )
  (model yag3d_MJ352W.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
